(module "LED-APA102-2020" (layer F.Cu) (tedit 5CE835A2)
  (descr "http://www.led-color.com/upload/201604/APA102-2020%20SMD%20LED.pdf")
  (tags "LED RGB SPI")
  (attr smd)
  (fp_text reference "D1" (at 0 2.11) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value "APA102" (at 0 -2) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 1.5 1.4) (end 0.5 1.4) (layer F.CrtYd) (width 0.05))
  (fp_line (start -0.5 1.4) (end -1.5 1.4) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.5 -1.4) (end -0.5 -1.4) (layer F.CrtYd) (width 0.05))
  (fp_line (start 0.5 -1.4) (end 1.5 -1.4) (layer F.CrtYd) (width 0.05))
  (fp_line (start 0.5 -1.58) (end 0.5 -1.4) (layer F.CrtYd) (width 0.05))
  (fp_line (start -0.5 -1.58) (end 0.5 -1.58) (layer F.CrtYd) (width 0.05))
  (fp_line (start -0.5 -1.4) (end -0.5 -1.58) (layer F.CrtYd) (width 0.05))
  (fp_line (start 0.5 1.58) (end 0.5 1.4) (layer F.CrtYd) (width 0.05))
  (fp_line (start -0.5 1.58) (end 0.5 1.58) (layer F.CrtYd) (width 0.05))
  (fp_line (start -0.5 1.4) (end -0.5 1.58) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1.5 -1.4) (end -1.5 1.4) (layer F.CrtYd) (width 0.05))
  (fp_line (start -0.5 -1) (end -1 -0.5) (layer F.Fab) (width 0.1))
  (fp_text user "%R" (at 0 0) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -1.2 -1.4) (end -0.5 -1.4) (layer F.SilkS) (width 0.12))
  (fp_line (start 1.5 -1.4) (end 1.5 1.4) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1 1) (end -1 -0.5) (layer F.Fab) (width 0.1))
  (fp_line (start 1 1) (end -1 1) (layer F.Fab) (width 0.1))
  (fp_line (start 1 -1) (end 1 1) (layer F.Fab) (width 0.1))
  (fp_line (start -0.5 -1) (end 1 -1) (layer F.Fab) (width 0.1))
  (pad "6" smd rect (at 0.85 -0.9) (size 0.8 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "4" smd rect (at 0.85 0.9) (size 0.8 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "5" smd rect (at 0.85 0) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "3" smd rect (at -0.85 0.9) (size 0.8 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "2" smd rect (at -0.85 0) (size 0.8 0.3) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "1" smd rect (at -0.85 -0.9) (size 0.8 0.5) (layers "F.Cu" "F.Paste" "F.Mask"))
  (model "${KIPRJMOD}/APA102.step"
    (offset (xyz 55.5 35.25 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
