(footprint "QFN-48-1EP_7x7mm_P0.5mm_EP5.3x5.3mm_ThermalVias_MR" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tedit 5DC5F6A5)
  (descr "QFN, 48 Pin (https://www.trinamic.com/fileadmin/assets/Products/ICs_Documents/TMC2041_datasheet.pdf#page=62), generated with kicad-footprint-generator ipc_noLead_generator.py")
  (tags "QFN NoLead")
  (property "Sheetfile" "Remote.kicad_sch")
  (property "Sheetname" "")
  (zone_connect 2)
  (attr smd)
  (fp_text reference "U7" (at 2.35 -4.95) (layer "F.SilkS")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 7705e9a7-8d84-410d-b2f3-d793d91b5f00)
  )
  (fp_text value "ESP32-PICO-D4" (at 0 4.8) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp bfbba12a-daed-4675-982a-77c43bac19b1)
  )
  (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab")
    (effects (font (size 1 1) (thickness 0.15)))
    (tstamp 47961ae4-c43b-4702-bdc7-45bd69e64f36)
  )
  (fp_line (start 3.135 -3.61) (end 3.61 -3.61) (layer "F.SilkS") (width 0.12) (tstamp 82260df7-7cb0-4a05-bc92-24745968f6f3))
  (fp_line (start 3.135 3.61) (end 3.61 3.61) (layer "F.SilkS") (width 0.12) (tstamp adfd5f8f-2d29-46d8-8047-03b2aaa9dc6e))
  (fp_line (start -3.61 3.61) (end -3.61 3.135) (layer "F.SilkS") (width 0.12) (tstamp b055493d-bf63-4196-98ab-412eab7fa898))
  (fp_line (start -3.135 3.61) (end -3.61 3.61) (layer "F.SilkS") (width 0.12) (tstamp c11947d4-e00d-4c9c-b2ed-b8a15919a2bf))
  (fp_line (start 3.61 3.61) (end 3.61 3.135) (layer "F.SilkS") (width 0.12) (tstamp f2b5f76c-63bf-4ac7-9fee-ca73aa63cdfd))
  (fp_line (start 3.61 -3.61) (end 3.61 -3.135) (layer "F.SilkS") (width 0.12) (tstamp fd40282b-8a6d-412a-a5db-a246efccae17))
  (fp_circle (center -3.6 -3.6) (end -3.45 -3.6) (layer "F.SilkS") (width 0.3) (fill none) (tstamp f6ce92d2-8f8a-4b34-be3d-a036cc80b0bf))
  (fp_line (start 4.1 4.1) (end 4.1 -4.1) (layer "F.CrtYd") (width 0.05) (tstamp 20c4528d-c018-4151-93b4-332a24de84d6))
  (fp_line (start -4.1 4.1) (end 4.1 4.1) (layer "F.CrtYd") (width 0.05) (tstamp 273f3a32-fc79-4d8b-ade3-2e64a1847a1a))
  (fp_line (start -4.1 -4.1) (end -4.1 4.1) (layer "F.CrtYd") (width 0.05) (tstamp 3021b803-8940-402a-a778-d13af1e71053))
  (fp_line (start 4.1 -4.1) (end -4.1 -4.1) (layer "F.CrtYd") (width 0.05) (tstamp ab59f9af-5f57-40d6-b894-bbb87c406520))
  (fp_line (start -3.5 3.5) (end -3.5 -2.5) (layer "F.Fab") (width 0.1) (tstamp 4e4f049b-fc43-42b3-8b80-d04ca9f29b1e))
  (fp_line (start 3.5 3.5) (end -3.5 3.5) (layer "F.Fab") (width 0.1) (tstamp 59a8f64b-8fa0-449d-ba41-95b41fdbddd7))
  (fp_line (start 3.5 -3.5) (end 3.5 3.5) (layer "F.Fab") (width 0.1) (tstamp 9951cc79-31d0-49eb-b143-5a3b2b8e28cf))
  (fp_line (start -3.5 -2.5) (end -2.5 -3.5) (layer "F.Fab") (width 0.1) (tstamp b997296a-33bd-49a5-b806-17018dfe5f0a))
  (fp_line (start -2.5 -3.5) (end 3.5 -3.5) (layer "F.Fab") (width 0.1) (tstamp ede8250d-4f07-4a9e-ba45-882b5295db66))
  (pad "" smd roundrect (at 1.8 0.6) (size 1.026341 1.026341) (layers "F.Paste") (roundrect_rratio 0.2435837602)
    (zone_connect 2) (tstamp 0045943e-6df3-40ca-9104-3e32ef1c2361))
  (pad "" smd roundrect (at -0.6 -0.6) (size 1.026341 1.026341) (layers "F.Paste") (roundrect_rratio 0.2435837602)
    (zone_connect 2) (tstamp 12920999-1739-4177-bd30-7526c2a7c154))
  (pad "" smd roundrect (at -1.8 0.6) (size 1.026341 1.026341) (layers "F.Paste") (roundrect_rratio 0.2435837602)
    (zone_connect 2) (tstamp 16a0886d-1c6d-443d-87b7-0ca2476ace0b))
  (pad "" smd roundrect (at 0.6 0.6) (size 1.026341 1.026341) (layers "F.Paste") (roundrect_rratio 0.2435837602)
    (zone_connect 2) (tstamp 1d0c3d71-94ac-4b17-b2b8-aa5c7cdf4be0))
  (pad "" smd roundrect (at 0.6 -1.8) (size 1.026341 1.026341) (layers "F.Paste") (roundrect_rratio 0.2435837602)
    (zone_connect 2) (tstamp 2ab4815d-1487-4c66-a3f2-b99a62a51a0c))
  (pad "" smd roundrect (at -1.8 -1.8) (size 1.026341 1.026341) (layers "F.Paste") (roundrect_rratio 0.2435837602)
    (zone_connect 2) (tstamp 40c666dc-c058-4f23-89c9-623d332d7fec))
  (pad "" smd roundrect (at 1.8 -0.6) (size 1.026341 1.026341) (layers "F.Paste") (roundrect_rratio 0.2435837602)
    (zone_connect 2) (tstamp 4b71632f-627e-4565-b89c-0a1a5f3303de))
  (pad "" smd roundrect (at -0.6 0.6) (size 1.026341 1.026341) (layers "F.Paste") (roundrect_rratio 0.2435837602)
    (zone_connect 2) (tstamp 5249604f-be81-4ccd-ae00-67c73a7140c7))
  (pad "" smd roundrect (at 1.8 -1.8) (size 1.026341 1.026341) (layers "F.Paste") (roundrect_rratio 0.2435837602)
    (zone_connect 2) (tstamp 6520ea53-1d97-441a-a4cc-165e29e56f17))
  (pad "" smd roundrect (at 0.6 -0.6) (size 1.026341 1.026341) (layers "F.Paste") (roundrect_rratio 0.2435837602)
    (zone_connect 2) (tstamp 7f7defbb-f8ca-4fd4-9a43-138509d73085))
  (pad "" smd roundrect (at 1.8 1.8) (size 1.026341 1.026341) (layers "F.Paste") (roundrect_rratio 0.2435837602)
    (zone_connect 2) (tstamp 8edec0bf-f2bf-45dd-bd87-83807f690a36))
  (pad "" smd roundrect (at -1.8 -0.6) (size 1.026341 1.026341) (layers "F.Paste") (roundrect_rratio 0.2435837602)
    (zone_connect 2) (tstamp 9ae5f0a0-fb8d-499b-80fe-cac6a10aca58))
  (pad "" smd roundrect (at 0.6 1.8) (size 1.026341 1.026341) (layers "F.Paste") (roundrect_rratio 0.2435837602)
    (zone_connect 2) (tstamp 9fd613eb-74ca-4f00-8cc9-4d57f3238a65))
  (pad "" smd roundrect (at -0.6 1.8) (size 1.026341 1.026341) (layers "F.Paste") (roundrect_rratio 0.2435837602)
    (zone_connect 2) (tstamp a6fdef24-a35e-45d8-a27c-f61032313fc2))
  (pad "" smd roundrect (at -0.6 -1.8) (size 1.026341 1.026341) (layers "F.Paste") (roundrect_rratio 0.2435837602)
    (zone_connect 2) (tstamp b77d62c4-d30c-4260-a609-2c7b29d578dd))
  (pad "" smd roundrect (at -1.8 1.8) (size 1.026341 1.026341) (layers "F.Paste") (roundrect_rratio 0.2435837602)
    (zone_connect 2) (tstamp f15ec748-ab3e-4223-8daa-eaf7a3ad412d))
  (pad "1" smd roundrect (at -3.28 -2.75) (size 0.5 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
    (zone_connect 2) (tstamp 43169ead-e3c0-48c3-a860-0de9bc10341e))
  (pad "2" smd roundrect (at -3.28 -2.25) (size 0.5 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
    (zone_connect 2) (tstamp b599b1ac-9d7d-4d52-8f1a-4087459782fa))
  (pad "3" smd roundrect (at -3.28 -1.75) (size 0.5 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
    (zone_connect 2) (tstamp d738e266-6392-45b8-9b25-c25c5e16601c))
  (pad "4" smd roundrect (at -3.28 -1.25) (size 0.5 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
    (zone_connect 2) (tstamp 1a375be6-2e7f-4324-bdf5-a43ab437db8e))
  (pad "5" smd roundrect (at -3.28 -0.75) (size 0.5 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
    (zone_connect 2) (tstamp 36dab2cd-cf91-4016-a054-c510a912b39b))
  (pad "6" smd roundrect (at -3.28 -0.25) (size 0.5 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
    (zone_connect 2) (tstamp 534c3c91-04fc-4e09-a61f-c57948ace1cf))
  (pad "7" smd roundrect (at -3.28 0.25) (size 0.5 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
    (zone_connect 2) (tstamp 0a32d12e-8b03-43fb-91a1-581adfc4aa57))
  (pad "8" smd roundrect (at -3.28 0.75) (size 0.5 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
    (zone_connect 2) (tstamp 9b50b460-2f13-4fc3-adc5-a634ae0b801a))
  (pad "9" smd roundrect (at -3.28 1.25) (size 0.5 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
    (zone_connect 2) (tstamp 41b51996-f7b3-46d6-93ff-b1e43ac3bed6))
  (pad "10" smd roundrect (at -3.28 1.75) (size 0.5 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
    (zone_connect 2) (tstamp 1f8f89f1-7da7-43cc-9d4d-16ef64d245a6))
  (pad "11" smd roundrect (at -3.28 2.25) (size 0.5 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
    (zone_connect 2) (tstamp 6853c369-dfab-411d-9705-ff1f204c3029))
  (pad "12" smd roundrect (at -3.28 2.75) (size 0.5 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
    (zone_connect 2) (tstamp cf47d1c7-f23d-4242-b05b-375e35556b2d))
  (pad "13" smd roundrect (at -2.75 3.28) (size 0.3 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
    (zone_connect 2) (tstamp 1bae595f-595e-4575-8ab1-a60f675617d7))
  (pad "14" smd roundrect (at -2.25 3.28) (size 0.3 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
    (zone_connect 2) (tstamp 17ee9082-dc06-4b77-83f9-48e6a8108154))
  (pad "15" smd roundrect (at -1.75 3.28) (size 0.3 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
    (zone_connect 2) (tstamp c9674c38-5c9b-4376-a39e-823857119235))
  (pad "16" smd roundrect (at -1.25 3.28) (size 0.3 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
    (zone_connect 2) (tstamp 8f55cf7d-a353-4bc7-a442-463d4176d317))
  (pad "17" smd roundrect (at -0.75 3.28) (size 0.3 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
    (zone_connect 2) (tstamp 55291fe4-d593-4e80-9423-adcaec667ad4))
  (pad "18" smd roundrect (at -0.25 3.28) (size 0.3 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
    (zone_connect 2) (tstamp a0b359bd-15d9-46ae-a6cd-5e13ecaab75f))
  (pad "19" smd roundrect (at 0.25 3.28) (size 0.3 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
    (zone_connect 2) (tstamp 88319470-3104-4470-b9fc-bf5aa9247624))
  (pad "20" smd roundrect (at 0.75 3.28) (size 0.3 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
    (zone_connect 2) (tstamp 9b849915-740e-482a-95d5-087d9f7bba9d))
  (pad "21" smd roundrect (at 1.25 3.28) (size 0.3 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
    (zone_connect 2) (tstamp 0630074a-3662-4f64-b4a8-3f79a8b6433c))
  (pad "22" smd roundrect (at 1.75 3.28) (size 0.3 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
    (zone_connect 2) (tstamp 5982fcae-2a3c-4fa6-86fc-4928642d130d))
  (pad "23" smd roundrect (at 2.25 3.28) (size 0.3 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
    (zone_connect 2) (tstamp 62444e9e-e8bb-4592-a0b7-1a8a3d45a7d0))
  (pad "24" smd roundrect (at 2.75 3.28) (size 0.3 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
    (zone_connect 2) (tstamp 08bc676c-3623-4434-b2e1-722cc349205a))
  (pad "25" smd roundrect (at 3.28 2.75) (size 0.5 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
    (zone_connect 2) (tstamp 08f94f28-3e54-4baa-b623-307c23eb2cee))
  (pad "26" smd roundrect (at 3.28 2.25) (size 0.5 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
    (zone_connect 2) (tstamp 28c12f52-c41f-4090-a4ee-5197bb52442b))
  (pad "27" smd roundrect (at 3.28 1.75) (size 0.5 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
    (zone_connect 2) (tstamp d9bdf50f-0ada-40f6-848e-6e604303ba49))
  (pad "28" smd roundrect (at 3.28 1.25) (size 0.5 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
    (zone_connect 2) (tstamp 9b19a0a3-0c4b-43e0-974c-2ea6f7585b65))
  (pad "29" smd roundrect (at 3.28 0.75) (size 0.5 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
    (zone_connect 2) (tstamp 29eb24df-25ea-4e19-a102-cbc938297edd))
  (pad "30" smd roundrect (at 3.28 0.25) (size 0.5 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
    (zone_connect 2) (tstamp 1923b88e-2573-4f06-bbe0-17c33dcc99e5))
  (pad "31" smd roundrect (at 3.28 -0.25) (size 0.5 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
    (zone_connect 2) (tstamp 18f910d5-9602-4f5c-b3eb-5cb354b6b26e))
  (pad "32" smd roundrect (at 3.28 -0.75) (size 0.5 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
    (zone_connect 2) (tstamp 8a735efc-f8ce-46c9-a802-5bf894cae6c5))
  (pad "33" smd roundrect (at 3.28 -1.25) (size 0.5 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
    (zone_connect 2) (tstamp 7fbb9aa9-3faa-4a59-9eee-77f7f27dc643))
  (pad "34" smd roundrect (at 3.28 -1.75) (size 0.5 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
    (zone_connect 2) (tstamp 7029b909-7155-45a6-afe0-edb4d8e853c5))
  (pad "35" smd roundrect (at 3.28 -2.25) (size 0.5 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
    (zone_connect 2) (tstamp f5498447-3b5c-4788-a427-e00b006f86c3))
  (pad "36" smd roundrect (at 3.28 -2.75) (size 0.5 0.3) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
    (zone_connect 2) (tstamp 25217a3e-da1d-44e5-bd8d-1b91d1c757de))
  (pad "37" smd roundrect (at 2.75 -3.28) (size 0.3 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
    (zone_connect 2) (tstamp 8a779b02-070b-4a04-b13c-91f13c535ef6))
  (pad "38" smd roundrect (at 2.25 -3.28) (size 0.3 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
    (zone_connect 2) (tstamp 5344680f-03d1-4cde-a774-d4313edf842a))
  (pad "39" smd roundrect (at 1.75 -3.28) (size 0.3 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
    (zone_connect 2) (tstamp 20880354-0997-4a10-bb7a-e9c51e1cf2bb))
  (pad "40" smd roundrect (at 1.25 -3.28) (size 0.3 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
    (zone_connect 2) (tstamp cc85cb1b-014f-40b7-a167-38e00819e7d1))
  (pad "41" smd roundrect (at 0.75 -3.28) (size 0.3 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
    (zone_connect 2) (tstamp 6fd0397c-3082-40c3-ac95-4e5e3920f842))
  (pad "42" smd roundrect (at 0.25 -3.28) (size 0.3 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
    (zone_connect 2) (tstamp c09a90d9-8382-44b4-a5d8-e0328a8fefe0))
  (pad "43" smd roundrect (at -0.25 -3.28) (size 0.3 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
    (zone_connect 2) (tstamp 05582249-0958-41ac-b6c5-ba9aedd73e8b))
  (pad "44" smd roundrect (at -0.75 -3.28) (size 0.3 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
    (zone_connect 2) (tstamp 682599c1-1fc4-4d2f-b481-05eae628df9d))
  (pad "45" smd roundrect (at -1.25 -3.28) (size 0.3 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
    (zone_connect 2) (tstamp e65fc06d-b11d-480a-8c45-89374b60242d))
  (pad "46" smd roundrect (at -1.75 -3.28) (size 0.3 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
    (zone_connect 2) (tstamp 6c9019a7-9971-4994-9603-b324ddfe473d))
  (pad "47" smd roundrect (at -2.25 -3.28) (size 0.3 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
    (zone_connect 2) (tstamp d3778f2d-cdf8-4efc-bba6-59156e3e95d6))
  (pad "48" smd roundrect (at -2.75 -3.28) (size 0.3 0.5) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.1)
    (zone_connect 2) (tstamp 8929094a-93b6-4f58-9014-aeac5138770c))
  (pad "49" thru_hole circle (at -1.2 -1.2) (size 0.5 0.5) (drill 0.25) (layers *.Cu)
    (zone_connect 2) (tstamp 051e6a54-8b5f-4265-ac56-3d6377b7ae04))
  (pad "49" thru_hole circle (at 1.2 1.2) (size 0.5 0.5) (drill 0.25) (layers *.Cu)
    (zone_connect 2) (tstamp 0b607888-5922-47fd-a47e-eca703a66daf))
  (pad "49" thru_hole circle (at 1.2 2.4) (size 0.5 0.5) (drill 0.25) (layers *.Cu)
    (zone_connect 2) (tstamp 1ec80c71-4fe2-4252-82fa-e619288c9877))
  (pad "49" thru_hole circle (at -1.2 0) (size 0.5 0.5) (drill 0.25) (layers *.Cu)
    (zone_connect 2) (tstamp 202a8353-df0d-4531-91d0-108aff3c0a03))
  (pad "49" thru_hole circle (at 2.4 2.4) (size 0.5 0.5) (drill 0.25) (layers *.Cu)
    (zone_connect 2) (tstamp 2232b45e-f070-457d-a8d9-4a472a7f03a7))
  (pad "49" thru_hole circle (at 1.2 -2.4) (size 0.5 0.5) (drill 0.25) (layers *.Cu)
    (zone_connect 2) (tstamp 288719ec-f74c-43db-8f67-370e454ae9d1))
  (pad "49" thru_hole circle (at 2.4 -2.4) (size 0.5 0.5) (drill 0.25) (layers *.Cu)
    (zone_connect 2) (tstamp 2f4af0f5-60ee-4658-a6f6-a57240013afb))
  (pad "49" thru_hole circle (at -2.4 0) (size 0.5 0.5) (drill 0.25) (layers *.Cu)
    (zone_connect 2) (tstamp 4809c405-e5ae-41a4-80b0-e037558edb1f))
  (pad "49" thru_hole circle (at -1.2 2.4) (size 0.5 0.5) (drill 0.25) (layers *.Cu)
    (zone_connect 2) (tstamp 596804b1-365f-4417-8172-048aa1582c66))
  (pad "49" thru_hole circle (at 0 -1.2) (size 0.5 0.5) (drill 0.25) (layers *.Cu)
    (zone_connect 2) (tstamp 67dedd75-1029-4a6e-9dab-32184da018ce))
  (pad "49" thru_hole circle (at 0 0) (size 0.5 0.5) (drill 0.25) (layers *.Cu)
    (zone_connect 2) (tstamp 69fe4f3c-b317-474e-b45a-f7ddf0d8ef36))
  (pad "49" thru_hole circle (at 0 2.4) (size 0.5 0.5) (drill 0.25) (layers *.Cu)
    (zone_connect 2) (tstamp 6b24ae74-c345-494f-91df-5c58a885337b))
  (pad "49" thru_hole circle (at 0 1.2) (size 0.5 0.5) (drill 0.25) (layers *.Cu)
    (zone_connect 2) (tstamp 7157b059-b234-496a-934d-3c9f2a03238d))
  (pad "49" thru_hole circle (at 2.4 1.2) (size 0.5 0.5) (drill 0.25) (layers *.Cu)
    (zone_connect 2) (tstamp 7a9cb4f1-60bb-45ea-ba68-a9c0fb7a9bc9))
  (pad "49" thru_hole circle (at -2.4 -2.4) (size 0.5 0.5) (drill 0.25) (layers *.Cu)
    (zone_connect 2) (tstamp 849b7cbf-4c82-4c26-9592-c5ef2533b3a5))
  (pad "49" thru_hole circle (at 1.2 -1.2) (size 0.5 0.5) (drill 0.25) (layers *.Cu)
    (zone_connect 2) (tstamp 8a02b4b3-1b58-40f0-86a5-625289d05d8d))
  (pad "49" thru_hole circle (at -2.4 1.2) (size 0.5 0.5) (drill 0.25) (layers *.Cu)
    (zone_connect 2) (tstamp 8e1b528e-c31b-4ab6-aac6-3a9bab7ce9ee))
  (pad "49" thru_hole circle (at 2.4 0) (size 0.5 0.5) (drill 0.25) (layers *.Cu)
    (zone_connect 2) (tstamp a1ed522d-538c-4f12-9667-ae046de55c2b))
  (pad "49" thru_hole circle (at -2.4 2.4) (size 0.5 0.5) (drill 0.25) (layers *.Cu)
    (zone_connect 2) (tstamp a5c015ed-d7a2-4d0c-b946-8d5a2d23b303))
  (pad "49" thru_hole circle (at 1.2 0) (size 0.5 0.5) (drill 0.25) (layers *.Cu)
    (zone_connect 2) (tstamp ab3f2f85-748b-4efb-bbfa-c2c5600046ba))
  (pad "49" thru_hole circle (at 0 -2.4) (size 0.5 0.5) (drill 0.25) (layers *.Cu)
    (zone_connect 2) (tstamp abeb7f94-d70e-4476-a09f-2122ade2d151))
  (pad "49" thru_hole circle (at 2.4 -1.2) (size 0.5 0.5) (drill 0.25) (layers *.Cu)
    (zone_connect 2) (tstamp afdf5e42-a0f9-46df-b6cd-bff7f5608140))
  (pad "49" thru_hole circle (at -1.2 -2.4) (size 0.5 0.5) (drill 0.25) (layers *.Cu)
    (zone_connect 2) (tstamp c9944f72-3222-4c01-ac64-0ee036802ce6))
  (pad "49" smd rect (at 0 0) (size 5.3 5.3) (layers "F.Cu" "F.Mask")
    (zone_connect 2) (tstamp ca3359f2-cf00-443e-b2ba-f22a094ec451))
  (pad "49" smd rect (at 0 0) (size 5.3 5.3) (layers "B.Cu")
    (zone_connect 2) (tstamp d006a54e-4e12-47c0-a16a-23930d48db30))
  (pad "49" thru_hole circle (at -2.4 -1.2) (size 0.5 0.5) (drill 0.25) (layers *.Cu)
    (zone_connect 2) (tstamp f7af55fc-8270-4072-ac7d-4585563010b0))
  (pad "49" thru_hole circle (at -1.2 1.2) (size 0.5 0.5) (drill 0.25) (layers *.Cu)
    (zone_connect 2) (tstamp f7fc7b74-5737-4bf4-8d03-c6eb7cbf7fe0))
  (model "${KICAD6_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/QFN-48-1EP_7x7mm_P0.5mm_EP5.3x5.3mm.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
